Space demands of human were determined, among the others, by Le Corbusier with figure called:

:r1 Modulor

:r2 Renaissance man

:r3 Vitruvius man

:r1 ok 2

:r2 -1

:r3 -1

--

The apartment social zone is made up by following rooms:

:r1 interior corridor, bedroom, children´s room

:r2 dining room, interior corridor, children´s room

:r3 dining room, kitchen, hall

:r1 -1

:r2 -1

:r3 ok 2

--

Space for guest operation in accommodation facility is:

:r1 restaurant section

:r2 reception office

:r3 parking lot

:r1 ok 2

:r2 -1

:r3 -1

--

Division of education facilities according to the movement system in the building:

:r1 dynamic system, statistical system, semi-statistical system

:r2 dynamic system, static system, semi-dynamic system

:r3 dynamic system, static system, semi-static system

:r1 -1

:r2 ok 2

:r3 -1

--

The mosque is:

:r1 Buddhist spiritual building that is circumvented

:r2 Muslim spiritual and educational building

:r3 Hinduistic educational building

:r1 -1

:r2 ok 2

:r3 -1

--

Basilica in ancient Greece is:

:r1 settlement church

:r2 marketplace or a courtroom

:r3 the space, where the archons officiate

:r1 -1

:r2 -1

:r3 ok 2

--

Among operating areas in spa treatment are not:

:r1 rooms for clients

:r2 space for souvenirs

:r3 social hall

:r1 -1

:r2 ok 2

:r3 -1

--

Large office space contains:

:r1 5 – 50 workplaces

:r2 11 or more workplaces

:r3 1 – 10 workplaces

:r1 -1

:r2 ok 2

:r3 -1

--

The area of large-sized breed of sheep must contain:

:r1 bathing pool

:r2 disinfection passage

:r3 harness

:r1 ok 2

:r2 -1

:r3 -1

--

Free production equipment is characterized by:

:r1 uncovered technological equipment

:r2 low object height

:r3 great built-up area

:r1 ok 2

:r2 -1

:r3 -1

Building requirements are:

:r1 Health requirements, psychic requirements, safety requirements, structural requirements, ecological requirements, ethical requirements

:r2 Health requirements, psychological requirements, safety requirements, structural requirements, economical requirements, aesthetic requirements

:r3 Health requirements, psychic requirements, safety requirements, structural requirements, ecological requirements, aesthetic requirements

:r1 -1

:r2 ok 2

:r3 -1

--

Among composition elements, we don´t find:

:r1 asymmetry

:r2 tectonics

:r3 typization

:r1 -1

:r2 -1

:r3 ok 2

--

Space demands of human were determined, among the others, by Leonardo da Vinci with figure called:

:r1 Modulor

:r2 Modular

:r3 Vitruvius man

:r1 -1

:r2 -1

:r3 ok 2

--

The apartment rest zone is made up by following rooms:

:r1 interior corridor, bedroom, children´s room

:r2 dining room, interior corridor, children´s room

:r3 dining room, kitchen, bedroom

:r1 ok 2

:r2 -1

:r3 -1

--

Difference between family house and apartment building and defined in legislation is in:

:r1 number of housing units

:r2 size of the built-up area

:r3 aesthetic design

:r1 ok 2

:r2 -1

:r3 -1

--

The main space/s in apartment building is/are:

:r1 staircase

:r2 technical equipment

:r3 flats

:r1 -1

:r2 -1

:r3 ok 2

--

The loft is:

:r1 accessible interior above the last above-ground floor, defined by the truss construction and other building structures, designed for purposeful use

:r2 accessible interior above the last above-ground floor, defined by the truss construction and other building structures, designed without a purpose

:r3 inaccessible interior above the last above-ground floor, defined by the truss construction and other building structures, designed without a purpose

:r1 ok 2

:r2 -1

:r3 -1

--

Orientation of spaces for guests at the accommodation facility should be mostly towards following cardinal directions:

:r1 S, eventually E, W

:r2 E, eventually SE, NE

:r3 N, eventually NE, NW

:r1 ok 2

:r2 -1

:r3 -1

--

Among spaces for staff operation in accommodation facilities is:

:r1 guest services

:r2 reception office

:r3 parking for staff

:r1 -1

:r2 ok 2

:r3 -1

--

Catering facilities are divided into:

:r1 open and purposeful

:r2 open and enclosed

:r3 public and enclosed

:r1 ok 2

:r2 -1

:r3 -1

Spaces of sports facilities are divided into:

:r1 spaces for athletes, spaces for staff, spectators spaces

:r2 spaces for athletes, spectators spaces, complementary spaces

:r3 sports area, spaces for staff, technical facilities

:r1 -1

:r2 ok 2

:r3 -1

--

Primary schools in the Czech Republic are placed:

:r1 so that children can be transported to school weekly

:r2 so that the school will be in the distance enabling walking

:r3 so that school will be accessible from the place of parents´ work

:r1 -1

:r2 ok 2

:r3 -1

--

Division of education facilities according to the movement system in the building:

:r1 dynamic system, statistical system, semi-statistical system

:r2 dynamic system, static system, semi-static system

:r3 dynamic system, static system, semi-dynamic system

:r1 -1

:r2 -1

:r3 ok 2

--

In buildings for culture, the portal is:

:r1 a fixed construction that separates the spectator from secondary areas

:r2 a movable construction that carries lighting for the stage

:r3 a fixed or movable construction that frames the spectator's optical perception of the stage

:r1 -1

:r2 -1

:r3 ok 2

--

Stupa is:

:r1 Buddhist spiritual building that is circumvented

:r2 Jewish spiritual building

:r3 Hindu spiritual structure of tower character

:r1 ok 2

:r2 -1

:r3 -1

--

Basilica in ancient Greece is:

:r1 settlement church

:r2 the space, where the archons officiate

:r3 marketplace or a courtroom

:r1 -1

:r2 -1

:r3 ok 2

--

In Elizabethan theater space, the stage is surrounded by auditorium from:

:r1 one side

:r2 two sides

:r3 three sides

:r1 -1

:r2 -1

:r3 ok 2

--

Among primary operating areas in ambulant care facilities are not:

:r1 sanitary facilities for staff

:r2 toilet for patients

:r3 waiting room

:r1 ok 2

:r2 -1

:r3 -1

--

Among operating areas in spa treatment are:

:r1 space for souvenirs

:r2 catering part

:r3 parks and gardens

:r1 -1

:r2 ok 2

:r3 -1

--

The purpose of polyclinic in the hospital campus is:

:r1 ambulant treatment of patients

:r2 long-term treatment of bed patients

:r3 complicated patients surgery operations

:r1 ok 2

:r2 -1

:r3 -1

The criterion for division of buildings for the trade by size is:

:r1 2000 m2

:r2 2200 m2

:r3 2500 m2

:r1 -1

:r2 -1

:r3 ok 2

--

Among the requirements for the location of objects for trade and services are not:

:r1 aesthetic harmonization of objects with surroundings

:r2 technical requirements and hygienic requirements (lighting, thermal and acoustic comfort, air exchange requirements, psychological comfort of working and visitors, aesthetic requirements, etc.)

:r3 traffic accessibility of localities

:r1 ok 2

:r2 -1

:r3 -1

--

In primary part of functional units of buildings for trade is:

:r1 entrance part

:r2 administration

:r3 warehouses

:r1 ok 2

:r2 -1

:r3 -1

--

Administrative buildings are divided in terms of access in:

:r1 free access of persons and with reception

:r2 free access of persons and forbidden access

:r3 with limited access to persons and with unrestricted access

:r1 -1

:r2 -1

:r3 ok 2

--

Cellular office contains:

:r1 2 – 15 workplaces

:r2 15 and more workplaces

:r3 1 – 10 workplaces

:r1 -1

:r2 -1

:r3 ok 2

--

Among gardening buildings are not:

:r1 fruit dryers

:r2 foil beds

:r3 greenhouses

:r1 ok 2

:r2 -1

:r3 -1

--

Storage of grain:

:r1 in buckets on exterior paved area

:r2 in buckets on paved area sheltered by shelter

:r3 in heaps on floors

:r1 -1

:r2 -1

:r3 ok 2

--

The area of large-sized breed of pigs, unlike the area for large-sized breed of dairy cows, requires:

:r1 veterinarian background

:r2 disinfection passage

:r3 dairy

:r1 -1

:r2 ok 2

:r3 -1

--

Basic factors for location of industrial buildings are:

:r1 availability of raw materials and of workforce, proximity to the market / outlet

:r2 sufficient space and availability of workforce

:r3 sufficient space, possibilities of landscape plan and proximity of the residential area

:r1 ok 2

:r2 -1

:r3 -1

--

Division of industrial production in the Czech Republic:

:r1 light, medium-heavy, heavy and special

:r2 light, medium-heavy and heavy

:r3 light, medium, heavy and strange

:r1 ok 2

:r2 -1

:r3 -1